**Table of figures**

Figure 1 : IoT devices vs human population…………………………………………………………………………………………………………………..…….p1  
Figure 2 : Usual approach very simple schematic……………………………………………………..………………………………………………..……….p2  
Figure 3 : Peer-to-peer approach very simple schematic…………………………………………………………………………………………....………p3  
Figure 4 : CRDT add-min set schematic example………………………………………………………………………………………………….……………..p4  
Figure 5 : Lasp official logo…………………………………………………………………………………………………………………………..…………..…………p6  
Figure 6 : ORSWOT general structure example…………………………………..…………………………………………………………..…………….…….p7  
Figure 7 : Orswot element addition example………………………………………………………………………………………………………..…….………p8  
Figure 8 : Orswot element removal example……………………………………………………………………………………………………………..…….…p8  
Figure 9 : Orswot states merging example……………………………………………………………………………………………………….……..…..….….p9  
Figure 10 : Orswot timeline example…………………………………………………………………………………………………………………..………..…….p9  
Figure 11 : launchContinuousMeasures debug=false real example………………………………………………………………………………...…p15  
Figure 12 : launchContinuousMeasures debug=true real example……….……………………………………………………………………….…..p16  
Figure 13 : getSystemConvergenceInfos real example……………………………………………………………………………………………………….p17  
Figure 14 : getSystemConvergenceTime real example……………………………………………………………………………………………………….p17  
Figure 15 : getSystemWorstNodeId real example………………………………………………………………………………………………………………p18  
Figure 16 : getSystemRoundTrip real example…………………………………………………………………………………………………………………..p18  
Figure 17 : getSystemNetworkUsage real example……………………………………………………………………………………………………………p19  
Figure 18 : getIndividualConvergenceTimes real example…………………………………………………………………………………………………p19  
Figure 19 : getConvergenceTime real example………………………………………………………………………………………………………………….p20  
Figure 20 : setStateInterval real example…………………………………………………………………………………………………….…………………….p21  
Figure 21 : getStateInterval real example………………………………………………………………………………………………………………………….p21  
Figure 22: Difference between Continuous updates interval and State sending interval…………………………………………………..p31  
Figure 23 : Graphs convergence time and network usage for different cluster size (nodes adding 10 elements each).……..p33  
Figure 24 : Graphs convergence time and network usage for different cluster size (nodes adding 100 elements each)…....p35  
Figure 25 : Graphs convergence time and network usage for different cluster size (nodes removing 10,100 elements)……p36  
Figure 26 : Graphs convergence time and network usage for different nodes distance (nodes adding 10 elements each)..p38  
Figure 27 : Graphs convergence time and network usage for different CRDT content (5 nodes adding elements).……………p39  
Figure 28 : Graphs convergence time and network usage for different CRDT content (5 nodes removing elements)……..…p40  
Figure 29 : Graph convergence time for different CRDT operation (5 nodes)………………………………………….…………………………p41  
Figure 30 : Graph network usage for different CRDT operation (5 nodes)………………………………………………………………………...p41  
Figure 31 : Graphs convergence time and network usage for different CRDT operation (10 nodes)………………………………....p42  
Figure 32 : Graphs Impact of partition on convergence time and network usage (on a 5 nodes cluster)……………………………p44  
Figure 33 : Graphs convergence time and network usage for a partitioned node (5 nodes cluster)…………………………………..p45  
Figure 34 : Graph convergence time for continuous updates at 2 updates/sec (5 nodes cluster)………………………………………p47  
Figure 35 : Overviews convergence time for continuous updates at different speeds (5 nodes)……………………………………….p49  
Figure 36 : Graph convergence time for different state\_intervals (5 nodes)……………………………………………………………………..p51  
Figure 37 : Graph Network usage for different state\_intervals (5 nodes)………………………………………………………………………….p51  
Figure 38 : Developed tools real usage example……………………………………………………………………………………………………………….p54